*********************************************************************************
                       GMxAGxx 12L EC RELEASE NOTE

*********************************************************************************
---------------------------------------------------------------------------------
2022/5/7                     EC Version 1.10.xx                    Owner: Cheng Sun
---------------------------------------------------------------------------------
File name: GMxAGxx_11.000  	(IDM/IDY/IDP)              (Checksum = 0x17AD10B)
File name: GMxAGxx_11.030	(IDO)                      (Checksum = 0x17B0410)
File name: GMxAGxx_11.079 	(IDW)                      (Checksum = 0x1778ADA)
File name: GMxAGxx_11.080	(IDN)			   		   (Checksum = 0x17AC878)
File name: GMxAGxx_11.089   (IDN + KMCW750)		       (Checksum = 0x17AC881)
Cypress PD FW version: 1.04

[Change item]:
1.  Fix DDS LCD brightness adjustment in NVIDIA control panel dgpu only.





[Important]:
N/A


Note(For manufacture): 

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF


---------------------------------------------------------------------------------
2022/4/25                     EC Version 1.09.xx                    Owner: Cheng Sun
---------------------------------------------------------------------------------
File name: GMxAGxx_10.900  	(IDM/IDY/IDP)              (Checksum = 0x17AF94B)
File name: GMxAGxx_10.930	(IDO)                      (Checksum = 0x17B2B82)
File name: GMxAGxx_10.979 	(IDW)                      (Checksum = 0x1779E07)
File name: GMxAGxx_10.980	(IDN)			   		   (Checksum = 0x17ADBF4)
File name: GMxAGxx_10.989   (IDN + KMCW750)		       (Checksum = 0x17ADBFD)
Cypress PD FW version: 1.06

[Change item]:
1.  Update cypress PD FW to 1.06.





[Important]:
N/A


Note(For manufacture): 

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF


---------------------------------------------------------------------------------
2022/4/13                     EC Version 1.08.xx                    Owner: Cheng Sun
---------------------------------------------------------------------------------
File name: GMxAGxx_10.800  	(IDM/IDY/IDP)              (Checksum = 0x17AE04A)
File name: GMxAGxx_10.830	(IDO)                      (Checksum = 0x17B1281)
File name: GMxAGxx_10.879 	(IDW)                      (Checksum = 0x1778506)
File name: GMxAGxx_10.880	(IDN)			   		   (Checksum = 0x17AC2F3)
File name: GMxAGxx_10.889   (IDN + KMCW750)		       (Checksum = 0x17AC2FC)
Cypress PD FW version: 1.04

[Change item]:
1.  Update IDM Turbo mode PL=110W PL2=110W PL4=165,TCC offset:10 for Hansung.
2.	Fix thirdwave keyboard single key on function.




[Important]:
N/A


Note(For manufacture): 

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF


---------------------------------------------------------------------------------
2022/4/2                     EC Version 1.07.xx                    Owner: Cheng Sun
---------------------------------------------------------------------------------
File name: GMxAGxx_10.700  	(IDM/IDY/IDP)              (Checksum = 0x17AF75C)
File name: GMxAGxx_10.730	(IDO)                      (Checksum = 0x17B2993)
File name: GMxAGxx_10.779 	(IDW)                      (Checksum = 0x1777A9F)
File name: GMxAGxx_10.780	(IDN)			   		   (Checksum = 0x17AC485)
File name: GMxAGxx_10.789   (IDN + KMCW750)		       (Checksum = 0x17AC48E)
Cypress PD FW version: 1.04

[Change item]:
1.  Update IDP/Y Turbo modeTCC offset 10 PL1=75W PL2=75W PL4=130W ,IDM Turbo mode PL=110W PL2=110W for Hansung.
2.	Add Max OC level function for liqud.
3.	Fix usb power function.



[Important]:
N/A


Note(For manufacture): 

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF


---------------------------------------------------------------------------------
2022/3/31                     EC Version 1.06.xx                    Owner: Cheng Sun
---------------------------------------------------------------------------------
File name: GMxAGxx_10.600  	(IDM/IDY/IDP)              (Checksum = 0x17B71A2)
File name: GMxAGxx_10.630	(IDO)                      (Checksum = 0x17BA3D9)
File name: GMxAGxx_10.679 	(IDW)                      (Checksum = 0x177CD86)
File name: GMxAGxx_10.680	(IDN)			   		   (Checksum = 0x17B2083)
File name: GMxAGxx_10.689   (IDN + KMCW750)		       (Checksum = 0x17B208C)
Cypress PD FW version: 1.04

[Change item]:
1.  Fix the oppositeof the two keys  'end' and '-'.
2.	Fix power led on behavior .
3.	Fix gpu fan speed and cpu fan speed.
4.	Update 4s1p battery normal 15-100% PL1/PL2/PL4 35/35/40.
5.	Update 3s1p/3s2p battery normal  15-100% and protection 70-100% gpuDs D2.


[Important]:
N/A


Note(For manufacture): 

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF


---------------------------------------------------------------------------------
2022/3/18                     EC Version 1.05.xx                    Owner: Cheng Sun
---------------------------------------------------------------------------------
File name: GMxAGxx_10.500 	(IDM/IDY/IDP)              (Checksum = 0x17BDC16)
File name: GMxAGxx_10.530	(IDO)                      (Checksum = 0x17BE622)
File name: GMxAGxx_10.579 	(IDW)                      (Checksum = 0x1781440)
File name: GMxAGxx_10.580	(IDN)			   		   (Checksum = 0x17B9771)
File name: GMxAGxx_10.589   (IDN + KMCW750)		       (Checksum = 0x17B977A)
Cypress PD FW version: 1.04

[Change item]:
1.  Add IDN 3rd keyboard.
2.	Fix E6 charger input current setting  13.5A -230W and others not change.
3.	Add Fn+4 and OC virtual scancode function.
4.	Add GPU temperature condition in Fan lock,Remoter temp,Safety function.
5.	Fix OOB to set PL12.
6.	Change IDN CapsLock control way by using GPIO. 
7.	Fix the output of the mainFan and the secondFan. 
8.  Add E5 smartAPC the same with E6.

[Important]:
N/A


Note(For manufacture): 

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF


---------------------------------------------------------------------------------
2022/3/3                     EC Version 1.04.xx                    Owner: Cheng Sun
---------------------------------------------------------------------------------
File name: GMxAGxx_10.400 	(IDM/IDY/IDP)              (Checksum = 0x17D27AE)
File name: GMxAGxx_10.430	(IDO)                      (Checksum = 0x17D441E)
File name: GMxAGxx_10.479 	(IDW)                      (Checksum = 0x178F4B7)
File name: GMxAGxx_10.480	(IDN)			   		   (Checksum = 0x17CEBC0)
File name: GMxAGxx_10.489   (IDN + KMCW750)		       (Checksum = 0x17CE9D2)
Cypress PD FW version: 1.04

[Change item]:
1.  Move Hook_Read_OEM_Service to 5ms.
2.	Fix right fucntion to set  Pl1/Pl2 = 60 in TTMode.
3.	Update the function of wakuang.


[Important]:
N/A


Note(For manufacture): 

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF


---------------------------------------------------------------------------------
2022/2/21                     EC Version 1.03.xx                    Owner: Cheng Sun
---------------------------------------------------------------------------------
File name: GMxAGxx_10.300 	(IDM/IDY/IDP)              (Checksum = 0x17D0170)
File name: GMxAGxx_10.330	(IDO)                      (Checksum = 0x17D1BE2)
File name: GMxAGxx_10.379 	(IDW)                      (Checksum = 0x178B8F6)
File name: GMxAGxx_10.380	(IDN)			   		   (Checksum = 0x17CDE8C)
File name: GMxAGxx_10.389   (IDN + KMCW750)		       (Checksum = 0x17CD9C3)
Cypress PD FW version: 1.04

[Change item]:
1.  Update standard IDW Fantbl.
2.	Change backlight logic during MS.
3.	Add charge limit for mcj.
4.	Update MCJ IDY/IDW Fantbl.
5.	Update  PL1Level = 60 ,PL2Level = 60 in TTMode .
6.	Add the value of TargetDCR is 100% if  the value of TargetDCR over 100%. 

[Important]:
N/A


Note(For manufacture): 

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2022/1/22                     EC Version 1.02.xx                    Owner: Cheng Sun
---------------------------------------------------------------------------------
File name: GMxAGxx_10.200 	(IDM/IDY/IDP)              (Checksum = 0x17E0ED4)
File name: GMxAGxx_10.230	(IDO)                      (Checksum = 0x17E310F)
File name: GMxAGxx_10.279 	(IDW)                      (Checksum = 0x179D510)
File name: GMxAGxx_10.280	(IDN)			   		   (Checksum = 0x17DCF1D)
File name: GMxAGxx_10.289   (IDN + KMCW750)		       (Checksum = 0x17DCDA0)
Cypress PD FW version: 1.04

[Change item]:
1.  In DC mode turn on and pull GPIO12 until enter windows.

[Important]:
N/A


Note(For manufacture): 

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2022/1/21                     EC Version 1.01.xx                    Owner: Cheng Sun
---------------------------------------------------------------------------------
File name: GMxAGxx_10.100 	(IDM/IDY/IDP)              (Checksum = 0x17E1770)
File name: GMxAGxx_10.130	(IDO)                      (Checksum = 0x17E39AB)
File name: GMxAGxx_10.179 	(IDW)                      (Checksum = 0x179F155)
File name: GMxAGxx_10.180	(IDN)			   		   (Checksum = 0x17DD58A)
File name: GMxAGxx_10.189   (IDN + KMCW750)		       (Checksum = 0x17DD0C4)
Cypress PD FW version: 1.04

[Change item]:
1.	Update IDM CPU Tcc Offset = 10 in game and turbo mode.
2. 	Update Pump fan duty; Fan: 40%/50%/60% (Default = 60%).
3.	Update	E3/E6/E7/E8 230w/280w/330w APC on Low Level 45w/45w/150w.

[Important]:
N/A


Note(For manufacture): 

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2022/1/8                     EC Version 1.00.xx                    Owner: Cheng Sun
---------------------------------------------------------------------------------
File name: GMxAGxx_10.000 	(IDM/IDY/IDP)              (Checksum = 0x17E22B5)
File name: GMxAGxx_10.030	(IDO)                      (Checksum = 0x17E44F0)
File name: GMxAGxx_10.079 	(IDW)                      (Checksum = 0x17A15AF)
File name: GMxAGxx_10.180	(IDN)			   		   (Checksum = 0x17DEBC7)
File name: GMxAGxx_10.089   (IDN + KMCW750)		       (Checksum = 0x17DE7B8)
Cypress PD FW version: 1.04

[Change item]:
1.  KMCW750 keybaord switch "end" and "-".
2.	Update Fan logic.
3. 	Support Web camera write protect function .
4.	Update IDN Power behavior.
5.	Update MS power consumption calculation.
6.	Update APC on low level 30/30/150w,E6 battry boost for 5A，E6 charge current 13.5 -230W.


[Important]:
N/A


Note(For manufacture): 

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2022/1/4                     EC Version 0.20.xx                    Owner: Cheng Sun
---------------------------------------------------------------------------------
File name: GMxAGxx_02.000	(IDM/IDY/IDP)              (Checksum = 0x17E0BA3)
File name: GMxAGxx_02.030	(IDO)                      (Checksum = 0x17E1CEF)
File name: GMxAGxx_02.079 	(IDW)                      (Checksum = 0x179C9EC)
File name: GMxAGxx_02.080	(IDN)			   		   (Checksum = 0x17DF526)
File name: GMxAGxx_02.089   (IDN + KMCW750)		       (Checksum = 0x17DF022)
Cypress PD FW version: 1.04

[Change item]:
1. EC code completes the writing of oemservice data.


[Important]:
N/A


Note(For manufacture): 

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2021/12/24                     EC Version 0.19.xx                    Owner: Jimmy
---------------------------------------------------------------------------------
File name: GMxAGxx_01.900	(IDM/IDY/IDP)              (Checksum = 0x17A58B4)
File name: GMxAGxx_01.930	(IDO)                      (Checksum = 0x17A6936)
File name: GMxAGxx_01.979	(IDW)                      (Checksum = 0x1759604)
File name: GMxAGxx_01.980	(IDN)			   (Checksum = 0x179DD90)
File name: GMxAGxx_01.989	(IDN + KMCW750)		   (Checksum = 0x179D91A)
Cypress PD FW version: 1.04

[Change item]:
1. Fix IDN membrane keyboard get wrong matrix.


[Important]:
N/A


Note(For manufacture): 

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2021/12/24                     EC Version 0.18.xx                    Owner: Jimmy
---------------------------------------------------------------------------------
File name: GMxAGxx_01.800	(IDM/IDY/IDP)              (Checksum = 0x17A58B3)
File name: GMxAGxx_01.830	(IDO)                      (Checksum = 0x17A6935)
File name: GMxAGxx_01.879	(IDW)                      (Checksum = 0x1759603)
File name: GMxAGxx_01.880	(IDN)			   (Checksum = 0x17A3F28)
Cypress PD FW version: 1.04

[Change item]:
1. Enable Liquid Cooling fucntion.
2. Update IDM Fan table.
3. Update PD FW to Uniwill_GM7AG8M_6227_v0.1.04 version.
4. Update KMCW750 UK matrix.
5. KMCW750 KB support anti-ghosting key function. (only membrane area)
6. Modify led behavior of IDN.
7. Modify recharge voltage level.

[Important]:
N/A


Note(For manufacture): 

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF


---------------------------------------------------------------------------------
2021/12/13                     EC Version 0.17.xx                    Owner: Jimmy
---------------------------------------------------------------------------------
File name: GMxAGxx_01.700	(IDM/IDY/IDP/IDN)          (Checksum = 0x17C1431)
File name: GMxAGxx_01.730	(IDO)                      (Checksum = 0x17C146F)
File name: GMxAGxx_01.779	(IDW)                      (Checksum = 0x176DD28)
Cypress PD FW version: 1.03

[Change item]:
1. Remove GC6 workaround.
2. Update smart apc table.
3. Update KMCW750 matrix.

[Important]:
N/A


Note(For manufacture): 

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2021/12/03                     EC Version 0.16.xx                    Owner: Jimmy
---------------------------------------------------------------------------------
File name: GMxAGxx_01.600	(IDM/IDY/IDP/IDN)          (Checksum = 0x17B6DEF)
File name: GMxAGxx_01.630	(IDO)                      (Checksum = 0x17B6E2D)
File name: GMxAGxx_01.679	(IDW)                      (Checksum = 0x176C3E3)
Cypress PD FW version: 1.03

[Change item]:
1. Update KMCW750 KB matrix.
2. PD FW change to Uniwill_GM7AG8M_6227_v0.1.03 version.
3. Fix Bug 24657. keyboard didn't light up when key pressed.
4. Disable special current calculation method in modern standby mode.
5. Modify some key vaule of IDN membrane KB.

[Important]:
N/A


Note(For manufacture): 

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2021/11/25                     EC Version 0.15.xx                    Owner: Jimmy
---------------------------------------------------------------------------------
File name: GMxAGxx_01.500	(IDM/IDY/IDP/IDN)          (Checksum = 0x17BC0F7)
File name: GMxAGxx_01.530	(IDO)                      (Checksum = 0x17BC135)
File name: GMxAGxx_01.579	(IDW)                      (Checksum = 0x176B3A1)
File name: GMxAGxx_01.589	(IDN+Diode KB)             (Checksum = 0x17BBDF7)

[Change item]:
1. Modify Adaptor power calculation function.
2. EC will not send TP Scan code when system is in modern standby mode.
3. Update IDM Fan table. (version : R03, 2021/11/19)
4. Fix ec may not send turn KB backlight off command in modern standby mode. 
5. PD FW change to Uniwill_GM7AG8M_6227_v0.1.02 version.

[Important]:
N/A


Note(For manufacture): 

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2021/11/18                     EC Version 0.14.xx                    Owner: Jimmy
---------------------------------------------------------------------------------
File name: GMxAGxx_01.400	                           (Checksum = 0x17C0AE2)
File name: GMxAGxx_01.430	                           (Checksum = 0x17C0B20)
File name: GMxAGxx_01.479	                           (Checksum = 0x176D6F3)	

[Change item]:
1. Fixed 4s1p(7A) battery protection trigger value is incorrect.
2. Fixed Type C lost TBT device bug. (BugZilla : 23811)
3. PD FW change to Uniwill_GM7AG8M_6227_v0.1.00.bin
4. Change Four / Full Area keyboard smbus channel to Ch2.

[Important]:
N/A


Note(For manufacture): 
 	GMxAGxx_01.x00 for IDM / IDY / IDP / IDN
	GMxAGxx_01.x30 for IDO
	GMxAGxx_01.x79 for IDW

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2021/11/05                     EC Version 0.12.xx                    Owner: Jimmy
---------------------------------------------------------------------------------
File name: GMxAGxx_01.200	                           (Checksum = 0x17C78C2)
File name: GMxAGxx_01.230	                           (Checksum = 0x17C7900)
File name: GMxAGxx_01.279	                           (Checksum = 0x176F734)	

[Change item]:
1. Add IDN Fan table.
2. Add E6 and E8 board ID.
3. Update IDM Fan table.
4. Update Smart APC table. (support 280w and 330w).

[Important]:
1. 280w adaptor need BIOS support.
   Please use BIOS version B004 or above !!


Note(For manufacture): 
 	GMxAGxx_01.x00 for IDM / IDY / IDP / IDN
	GMxAGxx_01.x30 for IDO
	GMxAGxx_01.x79 for IDW

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2021/10/22                     EC Version 0.11.xx                    Owner: Jimmy
---------------------------------------------------------------------------------
File name: GMxAGxx_01.100	                           (Checksum = 0x17E3C8A)
File name: GMxAGxx_01.130	                           (Checksum = 0x17E3CC8)
File name: GMxAGxx_01.179	                           (Checksum = 0x1789FEA)	

[Change item]:
1. Low-Temp charge current all change to 768 mA. (Refer to EC setting_V1.9-201023)
2. Fan table update for IDM, IDY, IDP, IDW and IDO.
3. Modify ChargeTimer function.
4. 4s1p (BATRPHID13-4101) dischareg current limit change to 7.7A.
5. Update smart apc table.
6. EC Ram define updated.(Refer to EC_ACPI_Spec_v2.11.pdf)

[Important]:
1. Charge IC of B phase MB change to OZ26786. Do not flash it on the A phase MB!!


Note(For manufacture): 
 	GMxAGxx_00.x00 for IDM / IDY / IDP
	GMxAGxx_00.x30 for IDO
	GMxAGxx_00.x79 for IDW

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2021/09/17                     EC Version 0.02.xx                    Owner: Jimmy
---------------------------------------------------------------------------------
File name: GMxAGxx_00.200	                           (Checksum = 0x179DC43)
File name: GMxAGxx_00.230	                           (Checksum = 0x179DC81)
File name: GMxAGxx_00.279	                           (Checksum = 0x174A08F)	

[Change item]:
1. Enable PD FW upgrade function. (FW version : Uniwill_GH5AD2D_6227_v0.1.02)
2. Update Read SMBus Block function. (ITE suggestion)
3. Disable Power button function within 5 secs after shutting down.
4. Add App trigger PWRBTN# pin function in shell mode.

[Important]:
1. New spec add:  User can't use Power button to boot system within 5 secs after shutting down.


Note(For manufacture): 
 	GMxAGxx_00.x00 for IDM / IDY / IDP
	GMxAGxx_00.x30 for IDO
	GMxAGxx_00.x79 for IDW

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

---------------------------------------------------------------------------------
2021/09/01                     EC Version 0.01.xx                    Owner: Jimmy
---------------------------------------------------------------------------------
File name: GMxAGxx_00.100	                           (Checksum = 0x1DC9DDE)
File name: GMxAGxx_00.130	                           (Checksum = 0x1DC9E1C)
File name: GMxAGxx_00.179	                           (Checksum = 0x1D7379E)	

[Change item]:
N/A

[Important]:
1. First release for SMT
2. Source Code base on GMxTGxx.


Note(For manufacture): 
 	GMxAGxx_00.x00 for IDM / IDY / IDP
	GMxAGxx_00.x30 for IDO
	GMxAGxx_00.x79 for IDW

STD ROMID (default)
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

MCJ  ROMID (IDW/Y)
ROMID.exe set 0x04 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDP/Y) 
ROMID.exe set 0x08 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Thirdwave ROMID (IDO) 
ROMID.exe set 0x18 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDP/Y)  same as STD US/UK
ROMID.exe set 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Monster German ROMID (IDR/O/M)  
ROMID.exe set 0x09 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

XMG German ROMID (IDW/S/O/R/M)  
ROMID.exe set 0x0C 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF

Mechrevo ROMID
ROMID.exe set 0x07 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF 0xFF


 
